aut-num:            AS4242420122
as-name:            GRMML ExaBGP Anycast
descr:              Used to distribute anycast failover information
remarks:            No direct Peering!
remarks:            See AS4242420123 for peering and more information.
admin-c:            GRMML-DN42
tech-c:             GRMML-DN42
mnt-by:             GRMML-MNT
source:             DN42
